Release Version 6.6
Introduction:
Accelera™ Diagnostics is a Windows software application that works with Accelera™ Control Modules to:
1. Diagnose problems
2. Analyze and store historical information about the product
3. Modify operating parameters of the product
4. Enables users to download calibrations to supported products
 
New Enhancements:
iBCR Support
Updated iBCR Service Model Name: iBCR Service Model name has been updated to iBCR CM3670 BC101.
Support for New Parameter in iBCR Digital Dataplate: A new parameter, “Advertised Power” has been added to the Digital Dataplate screen.
Support for New Special Features: The Accelera™ Diagnostics now supports the “System Status” and “System Temperature” special features for “iBCR CM3670 BC101”.
ELFA3 v3.2
Work Order Support: The Accelera™ Diagnostics now supports Work Orders and Images for ELFA3 v3.2.
ELFA3 v3.1
SPEED Flashing Support: The users can now download and flash calibrations for ELFA3 v3.1 through SPEED.
e-Powertrain EPS CM2377 DS101:
ROMboot Flash Support: The Accelera™ Diagnostics now allows users to flash e-Powertrain EPS CM2377 DS101 while the SCM is in ROMboot state.
PCAS BES CM0196 EV114B
Support for R7 Parameters: The Accelera™ Diagnostics now supports Monitor as well as Override parameters for the R7 release of the SCM Software version for Meritor PCAS.
Support of Occurrence Counter: The users shall now be able to view First Occurrence Count and Last Occurrence Count for the Fault Codes that support Occurrence Count.
Bosch VCU:
              Certificate Download Support: The tool can now securely download certificates from the server and write them to the Bosch VCU as part of the provisioning process.
Base Tool:
Enhancements on Connection tab: 
· The Accelera™ Diagnostics tool now provides the ability to sort and filter the product list in the Manual Connection card. 
· The tool also provides a button to browse the network calibrations to save default search time.
Enhancements in Calibration:  The Accelera™ Diagnostics tool now displays a warning message if the user tries to change the ECM Code while flashing.
Alert on Low Battery Voltage: The Accelera™ Diagnostics tool now alerts users if the battery voltage is low for the connected system.


Newly supported products:
	BES CM2450 EV108B



Newly Supported Special Features:
	System Status

	System Temperature



Supported Adapters:
	Adapter Name
	Communication Type

	All RP1210c compliant adapters
	USB/Wi-Fi/Bluetooth


 

Device Specifications:
·        Operating System: Windows 10 and above
·        RAM:  16GB and above
·        Processor: Intel Core i5 Gen 8 and above
 
Known Issues:
1. Users will not be able to auto-detect “BES CM3591 EV116B” due to a calibration issue. So manual selection will be required.
2. In the case of iBCR CH2-850WM-A, the tool will display some DTCs as “unknown” due to module reporting undefined or unexpected fault codes. An update to the software shall resolve the issue.
3. Users will not be able to flash ELFA3 v3.1 using peak adapter. Users can continue to use Inline 7 to flash the same.
