Accelera™ Diagnostics - Release Version 6.7

Introduction:
Accelera™ Diagnostics is a Windows software application that works with Accelera™ Control Modules to:
1. Diagnose problems
2. Analyze and store historical information about the product
3. Modify operating parameters of the product
4. Enables users to download calibrations to supported products
 
New Enhancements:

iBCR Support
Simulator Support: The Accelera™ Diagnostics now provides simulator support for “iBCR CM3670 BC101”.
Audit Trail: The Accelera™ Diagnostics now supports Audit Trail for “iBCR CM3670 BC101”.

ESS BP97 ES116
Battery Dashboard: The Accelera™ Diagnostics now navigates user to the Battery Dashboard that displays all the possible battery packs in a BMS configuration. 

BES CM2450 EV108B:
New Feature Support: The Accelera™ Diagnostics tool now supports feature – XALT Battery Throughput for school buses.

PCAS BES CM0196 EV114B
Support Fault Timestamp: The Accelera™ Diagnostics displays “SCM Controller On Time”, “First Occurrence” and “Last Occurrence” for PCAS BES CM0196 product.

Base Tool:
Language Support: The Accelera™ Diagnostics tool now supports Japanese language.

Enhancements in Connection:  Enhanced auto-detect connection performance for quicker and more efficient device connectivity.

Enhancements in Calibration:  
1. The Accelera™ Diagnostics tool now displays an updated warning message to keep key switch “On” before user starts the flashing process.
2. The tool shall now warn the users to disconnect and reconnect back to enable full feature access after Romboot controller is flashed successfully. 
Enhancements in Error Messages: The tool now displays simplified warning messages across the tool for features like connection, Dataplate, Parameters, Calibration, Audit Trail and Faults.

Save Report Functionality Support: 
1. The tool shall now be able to save report of failed parameters while template transfer.
2. The tool shall now be able to save report during image creation if the controller returns a negative response for reading parameters or freeze frame data.
3. The tool shall now be able to save the failed save and restore parameters in the PDF report after restore process.
4. The tool shall now be able to export the faults in excel format in addition to the PDF format on Faults tab.

Support of New Help tab: The Accelera™ Diagnostics tool now display Help tab with “Contact Us” and “Release Notes” details included. 


Newly supported Feature:
	XALT Battery Throughput



Supported Adapters:
	Adapter Name
	Communication Type

	All RP1210c compliant adapters
	USB/Wi-Fi/Bluetooth


 
Device Specifications:
·        Operating System: Windows 10 and above
·        RAM:  16GB and above
·        Processor: Intel Core i5 Gen 8 and above
 
Known Issues:
1. Users will not be able to auto-detect “BES CM3591 EV116B” due to a calibration issue. So manual selection will be required.
2. In the case of iBCR CH2-850WM-A, the tool will display some DTCs as “unknown” due to module reporting undefined or unexpected fault codes. An update to the software shall resolve the issue.
3. Users will not be able to flash ELFA3 v3.1 using peak adapter. Users can continue to use Inline 7 to flash the same.
